Data Fied Def\_Req

| S.No. | Name | Type | Description |
| --- | --- | --- | --- |
| 1 | UIN or VID\* | >UIN generated should be of the length defined by the ADMIN. In absence of configured length policy, UIN generated should be of 12 digits >VID generated should contain the number of digits as configured by the ADMIN In absence of ADMIN configured length, VID generated should have 16 digits | UIN or Virtual ID |
| 2 | ver\* | NA | Version of the Authentication API |
| 3 | reqTime\* | DateTime - ISO 8601 | Timestamp at the time of request. This is in format “YYYY-MM- DDThh:mm:ss” (derived from ISO 8601).  Time standard - UTC |
| 4 | pinval | Admin Configurable length  Default - Numeric(6) | pinval set by the resident using the MOSIP portal |
|  |

|  |
| --- |
| Notes: |
| * \* denotes mandatory |
|  |

Data Fied Def\_Res

|  |  |  |  |
| --- | --- | --- | --- |
| S.No. | Name | Type | Description |
|  | Response Section | | |
| 1 | status | Character(1) | Result of pin storage request ‘y’ or ‘n’. |
| 2 | resTime | DateTime - ISO 8601 | Time stamp of response. This is in format “YYYY-MM- DDThh:mm:ss” (derived from ISO 8601).  Time standard - UTC |
| 3 | err | NA | Error codes and Error Messages as defined in the Error Messages Document |
| 4 | reqTime | NA | As received in the request |
| 5 | ver | NA | As received in the request |